%Error-PROCASSWIRE: t/t_lint_always_comb_bad.v:28: Procedural assignment to wire, perhaps intended var (IEEE 2017 6.5): 'temp1'
                                                 : ... In instance t
        temp1 = 'h0;
        ^~~~~
%Error-PROCASSWIRE: t/t_lint_always_comb_bad.v:30: Procedural assignment to wire, perhaps intended var (IEEE 2017 6.5): 'temp1'
                                                 : ... In instance t
        temp1 = (temp1_d1r - 'h1);
        ^~~~~
%Warning-ALWCOMBORDER: t/t_lint_always_comb_bad.v:31: Always_comb variable driven after use: 'mid'
                                                    : ... In instance t
      mid = (temp1_d1r == 'h0);   
      ^~~
                       ... Use "/* verilator lint_off ALWCOMBORDER */" and lint_on around source to disable this message.
%Error-PROCASSWIRE: t/t_lint_always_comb_bad.v:45: Procedural assignment to wire, perhaps intended var (IEEE 2017 6.5): 'temp1_d1r'
                                                 : ... In instance t
      temp1_d1r <= temp1;
      ^~~~~~~~~
%Error: Exiting due to
