%Error-PROCASSWIRE: t/t_lint_always_comb_bad.v:29:9: Procedural assignment to wire, perhaps intended var (IEEE 1800-2017 6.5): 'temp1'
                                                   : ... In instance t
   29 |         temp1 = 'h0;
      |         ^~~~~
                    ... For error description see https://verilator.org/warn/PROCASSWIRE?v=latest
%Error-PROCASSWIRE: t/t_lint_always_comb_bad.v:31:9: Procedural assignment to wire, perhaps intended var (IEEE 1800-2017 6.5): 'temp1'
                                                   : ... In instance t
   31 |         temp1 = (temp1_d1r - 'h1);
      |         ^~~~~
%Warning-ALWCOMBORDER: t/t_lint_always_comb_bad.v:32:7: Always_comb variable driven after use: 'mid'
                                                      : ... In instance t
   32 |       mid = (temp1_d1r == 'h0);   
      |       ^~~
                       ... Use "/* verilator lint_off ALWCOMBORDER */" and lint_on around source to disable this message.
%Error-PROCASSWIRE: t/t_lint_always_comb_bad.v:46:7: Procedural assignment to wire, perhaps intended var (IEEE 1800-2017 6.5): 'temp1_d1r'
                                                   : ... In instance t
   46 |       temp1_d1r <= temp1;
      |       ^~~~~~~~~
%Error: Exiting due to
