%Warning-MULTIDRIVEN: t/t_lint_multidriven_bad.v:20: Signal has multiple driving blocks with different clocking: 't.mem'
                      t/t_lint_multidriven_bad.v:26: ... Location of first driving block
      mem[a0] <= d1;
      ^~~
                      t/t_lint_multidriven_bad.v:23: ... Location of other driving block
      mem[a0] <= d0;
      ^~~
                      ... Use "/* verilator lint_off MULTIDRIVEN */" and lint_on around source to disable this message.
%Warning-MULTIDRIVEN: t/t_lint_multidriven_bad.v:18: Signal has multiple driving blocks with different clocking: 'out2'
                      t/t_lint_multidriven_bad.v:34: ... Location of first driving block
      out2[15:8] <= d0;
      ^~~~
                      t/t_lint_multidriven_bad.v:31: ... Location of other driving block
      out2[7:0] <= d0;
      ^~~~
%Error: Exiting due to
