%Warning-CDCRSTLOGIC: t/t_cdc_async_bad.v:27: Logic in path that feeds async reset, via signal: 't.rst2_bad_n'
   wire  rst2_bad_n = rst0_n | rst1_n;
                    ^
                      ... Use "/* verilator lint_off CDCRSTLOGIC */" and lint_on around source to disable this message.
%Warning-CDCRSTLOGIC:      See details in obj_vlt/t_cdc_async_bad/Vt_cdc_async_bad__cdc.txt
%Warning-CDCRSTLOGIC: t/t_cdc_async_bad.v:52: Logic in path that feeds async reset, via signal: 't.rst6a_bad_n'
   wire rst6a_bad_n = rst6_bad_n ^ $c1("0");   
                    ^
%Warning-CDCRSTLOGIC: t/t_cdc_async_bad.v:53: Logic in path that feeds async reset, via signal: 't.rst6b_bad_n'
   wire rst6b_bad_n = rst6_bad_n ^ $c1("1");
                    ^
%Error: Exiting due to
